1: main_power							reg.100
	  0 = all off
	  1 = all can be on (based on point 2 and point 5)
	101 = only zone 1
	102 = only zone 2
	...
	120 = only zone 20

2: power   status for the small part
3: dimmed  status for the small part
4: twinkle status for the small part

5: power   status for the large part				reg.101
6: dimmed  status for the large part				reg.102
7: twinkle status for the large part				reg.103


11: loop 1 status
	0 = continously full
	1 = full twinkling
	2 = dimmed twinkling
	3 = continuously soft
12: loop 1 min value
13: loop 1 max value dimmed
14: loop 1 max value full
15: loop 1 speed up dimmed
16: loop 1 speed up full
17: loop 1 speed down dimmed
18: loop 1 speed down full

POINT33#MIN:0#MAX:100000#DIVIDER:1000
POINT34#MIN:0#MAX:100000#DIVIDER:1000