::Set modbusmaster baudrate

::BAUD=9600
::BAUD=19200
BAUD=38400
::BAUD=57600
::BAUD=115200

::Set bit count and parity
::BITS=8n1
::BITS=8e1
::BITS=8o1
BITS=8n1
::BITS=8e2
::BITS=8o2

::Set modbus send delay in milliseconds (a delay before next request)
SENDDELAY=500

::Select if modbusdevices should be made automatically or manually
MODBUSDEVICES=AUTO
::MODBUSDEVICES=MANUAL

::If MODBUSDEVICES=AUTO selected, these settings do not have any affect if MODBUSDEVICES=MANUAL selected
::Select if modbusdevices should be combined making one larger modbusdevice with multiple registers
::Number defines max registers per query or set to FALSE if combining is not allowed
::COMBINE=FALSE
::COMBINE=10
::Set modbus timeout in milliseconds (only for autogenerated modbus devices)
TIMEOUT=400

::If MODBUSDEVICES=MANUAL selected modbus devices have to be defined manually, these settings do not have any affect if MODBUSDEVICES=AUTO selected
::MODBUSDEVICE=ADDRESS:1, STARTREG:0, COUNT:1,  TYPE:HOLDING, TIMEOUT:100

::SENDTEMPERATURE=ADDRESS:11, STARTREG:2018, TIMEOUT:100
::SENDREGISTERS=ADDRESS:10, STARTREG:2000, SOURCEREG:3007, COUNT:1, TIMEOUT:300
